


SECTION 09 84 33
Metro Rebound Acoustical Wall Panels

PART 1 GENERAL 
1.1  	SECTION INCLUDES
A. Metro Rebound perforated co-polymer wrapped fiberglass acoustical wall panels and accessories for wall installation.
1.2 	SUBMITTALS
A. Product Data: Manufacturer’s data sheet and installation instructions.
B. Samples: Submit, at minimum, a 4” x 4” sample for each type of specified acoustical panel. 
1.3 	QUALITY ASSURANCE
A. Qualifications:
1. Manufacturers: Provide acoustical wall panels from a single manufacturer.
2. Installers: Utilize an installer having demonstrated experience on projects of comparable size and complexity.
1.4 	DELIVERY, STORAGE, AND HANDLING
A. Storage and Handling Requirements:
1. Handle panels carefully to avoid any damage.
2. Store panels indoors in a clean, cool, dry place, and out of direct sunlight.
3. Store panels in a space where the ambient temperature and humidity conditions are being maintained at the levels indicated for the project when occupied for its intended use.
1.5  	SITE CONDITIONS
A. Ambient Conditions:
1. Maintain ambient temperature and humidity conditions at levels indicated for the project when occupied for its intended use.
2. Do not install products under environmental conditions outside manufacturer’s recommended limits.
B. Existing Conditions: Do not install wall panels until space is enclosed and weather proofed, and wet work is completely dry.
1.6 	WARRANTY
A. Provide manufacturer’s written product warranty per Section 01 77 00 – Closeout Procedures.
PART 2 PRODUCTS 
(Specifier Note: Red colored text below requires you to select an option before this specification can be completed. Options in red text are bound by parenthesis. Additional Metro Rebound information can be found on our website https://www.acousticalsurfaces.com/acoustical-wall-panels/metro-rebound-wall-panel.html)
2.1  	MANUFACTURERS
A. Acoustical Surfaces, Inc., 123 Columbia Court N, Chaska, MN 55318.
Phone: 952-448-5300. Fax: 952-448-2613. Website: www.acousticalsurfaces.com
2.2  	DESCRIPTION
A. [bookmark: _Hlk23860703]Product: Metro Rebound perforated co-polymer wrapped fiberglass acoustical wall panels by Acoustical Surfaces, Inc.
B. Product Options: 
1. [bookmark: _Hlk23860713][bookmark: _Hlk33780891]Panel Composition:	Glass fiberboard core with perforated co-polymer face
2. Panel Density:		6-7 lb pcf
3. Panel Thickness:	(1-1/16”) / (2-1/16”)
4. Panel Size:		1-1/16” thickness: 	(width up to 46” x length up to 116”)
 			2-1/16” thickness: 	(width up to 44” x length up to 114”) 
5. Edge Detail: 		Square – resin hardened
6. Finish:			(Standard finish options available for co-polymer face) / (Custom
 			fabric finish options available)
7. Mounting Method:	(Z-Clips) / (Impaling Clips with Adhesive) 
2.3 ACCESSORIES
A. Attachment hardware for wall panels as specified by manufacturer for installation.
PART 3 EXECUTION
3.1  	EXAMINATION
A. Verification of Conditions:
1. Examine surfaces scheduled to received furred out or directly attached acoustical units for unevenness, irregularities or dampness that would affect quality and execution of work. 
2. All wet work in the installation area must be complete, cured, and dry prior to installation.
3. Wall assembly shall be complete, inspected, and accepted before wall work begins. 
3.2 	INSTALLATION
A. Comply with manufacturer’s instructions and recommendations for installation of wall panels and with industry standards.
3.3 	CLEANING
A. Clean surfaces of wall panels per manufacturer’s instructions or recommendations.
B. Remove and replace damaged or discolored material and material that cannot be properly cleaned. 
3.4 PROTECTION 
A. Protect installed work from damage due to subsequent construction activity, including temperature and humidity limitations and dust control, so that the work will be without damage and deterioration at the time of acceptance by the owner. 
END OF SECTION


