SECTION 09 84 33

Sound SilencerTM dBA Acoustic Wall Panels

**PART 1 GENERAL**

1. **SECTION INCLUDES**
   1. Sound SilencerTM dBA acoustic wall panels and accessories for wall installation.
2. REFERENCES
   1. American Society for Testing and Materials (ASTM)
      1. ASTM E84: Standard Test Method for Surface Burning Characteristics of Building Materials.
      2. ASTM E90: Standard Test Method for Laboratory Measurement of Airborne Sound Transmission Loss of Building Partitions and Elements
      3. ASTM C423: Standard Test Method for Sound Absorption and Sound Absorption Coefficients by the Reverberation Room Method.
      4. ASTM E795: Standard Practices for Mounting Test Specimens During Sound Absorption Tests
   2. International Code Council (ICC)
      1. ICC IBC: International Building Code
3. **SUBMITTALS**
   1. Product Data: Manufacturer’s data sheet and installation instructions.
   2. Samples: Submit, at minimum, a 4” x 4” sample for each type of specified acoustical panel.
   3. Test Reports: Upon request, submit certified test reports to verify specified product performance.
4. **QUALITY ASSURANCE**
   1. Qualifications:
      1. Manufacturers: Provide acoustical wall panels from a single manufacturer.
      2. Installers: Utilize an installer having demonstrated experience on projects of comparable size and complexity.
   2. Performance Requirements:
      1. Surface Burning Characteristics: Acoustical panels to perform as specified when tested in accordance with ASTM E84. Acoustical panel surface burning performance should comply with the International Building Code and other local building code requirements.
      2. Acoustical Characteristics: Acoustical panels to perform as specified when tested in accordance with ASTM C423 and ASTM E90.
5. **DELIVERY, STORAGE, AND HANDLING**
   1. Storage and Handling Requirements:
      1. Handle panels carefully to avoid any damage.
      2. Store panels indoors in a clean, cool, dry place, and out of direct sunlight.
      3. Store panels in a space where the ambient temperature and humidity conditions are being maintained at the levels indicated for the project when occupied for its intended use.
6. **SITE CONDITIONS**
   1. Ambient Conditions:
      1. Maintain ambient temperature and humidity conditions at levels indicated for the project when occupied for its intended use.
      2. Do not install products under environmental conditions outside manufacturer’s recommended limits.
   2. Existing Conditions: Do not install wall panels until space is enclosed and weather proofed, and wet work is completely dry.
7. **WARRANTY**
   1. Provide manufacturer’s written product warranty per Section 01 77 00 – Closeout Procedures.

**PART 2 PRODUCTS**

(Specifier Note: Red colored text below requires you to select an option before this specification can be completed. Options in red text are bound by parenthesis. Additional Acousti-Board Ultra information can be found on our website <https://www.acousticalsurfaces.com/sound_silencer/dBA_panel.htm>)

1. **MANUFACTURERS**
   1. Acoustical Surfaces, Inc., 123 Columbia Court N, Chaska, MN 55318.  
      Phone: 952-448-5300. Fax: 952-448-2613. Website: www.acousticalsurfaces.com
2. **DESCRIPTION**
   1. Product: Sound SilencerTM dBA acoustic wall panels by Acoustical Surfaces, Inc.
   2. Product Options:
      1. Panel Composition: Semi-rigid porous expanded polypropylene acoustical bead foam
      2. Panel Thickness: (1”) / (2”)
      3. Panel Size: Nominal - (2’ x 2’) / (2’ x 4’)
      4. Edge Profile: Square
      5. Finish: (Charcoal) / (White)
      6. Mounting Method: (Direct Attachment) / (Adhesive)
   3. Product Performance:
      1. Acoustical Performance
         1. Noise Reduction Coefficient (NRC) per ASTM C423

|  |  |  |
| --- | --- | --- |
| Thickness | 1” | 2” |
| A Mount | 0.50 | 0.65 |

* + - 1. Sound Transmission Classification (STC) per ASTM E90

|  |  |  |
| --- | --- | --- |
| Thickness | 1” | 2” |
| STC | 6 | 7 |
| OITC | 5 | 6 |

* + 1. Surface Burning Performance
       1. Fire Rating per ASTM E84: Class A.

1. **ACCESSORIES**
2. Attachment hardware for wall panels as specified by manufacturer for installation.

**PART 3 EXECUTION**

1. **EXAMINATION**
   1. Verification of Conditions:
      1. Examine surfaces scheduled to received furred out or directly attached acoustical units for unevenness, irregularities or dampness that would affect quality and execution of work.
      2. All wet work in the installation area must be complete, cured, and dry prior to installation.
      3. Wall assembly shall be complete, inspected, and accepted before wall work begins.
2. **INSTALLATION**
3. Comply with manufacturer’s instructions and recommendations for installation of wall panels and with industry standards.
4. **CLEANING**
5. Clean surfaces of wall panels per manufacturer’s instructions or recommendations.
6. Remove and replace damaged or discolored material and material that cannot be properly cleaned.
7. **PROTECTION**
8. Protect installed work from damage due to subsequent construction activity, including temperature and humidity limitations and dust control, so that the work will be without damage and deterioration at the time of acceptance by the owner.

END OF SECTION